  Hi! As some users have trouble to prime the vacuum hose ( get air out of the hose ).
  I write up a simplified user guide to help users to save time searching the net for solution.

  Setup the vacuum body first.
  The vacuum is made up with three parts, body, head cover, and debris bag. The head just twist locks into place after you put in the debris bag.
  When you screw the cover on it clicks on, gentlely screwes it in more and heard a 2nd click. But do not over thighten it. The head cover may come off if it not twist locked properly.

  Attach the pole into the vacuum body. 
  Follow below steps:

  1. Insert the pole with the vacuum into water.
  2. With your arm hold the pole,  Submerge the hose vertically into the water slowly length by length with 2 hands
  3. You will see water and bubble coming out of the mouth of the hose when you reach the other end of the hose
  4. Hook this end into the the inlet of the pool ( take the skimmer off first if any )
  5. If there is 2 in-let in the pool, cover one to get more suction power with the small rubber piece ( the set comes with) in the other hole.
  6. Release any additional air by holding hose onto the OUTLET once pump is running. 
  
  Then it is ready to vacuum the pool.

  Other points to note:
  - Remember to clean your filter cartridge and the mesh bag after the vacuum
  - Be gentle with the mesh bag when cleaning it, as it is only single stitched to the rubber grommet 
  - When the suction power slows down, the bag may be full, take it out and clean it with garden hose
  - Do not lift the vacuum out of the water surface during the vacuum process, this will let air get into the vacuum
  - Be careful with the vacuum head as it is made of plastic and if you drop it or over tighten it could break/fracture
  
https://www.youtube.com/watch?v=HrFcsnbAQJ0  
Priming the vacuum hose starts from 3:36. check this. I could help,

